# Bally Nip It

## Physical Setup

* Level Machine, per factory recommendation
* Ear Plug Tilt Hack if it makes sense
* Verify Tilt Sensitivity – should be sensitive, tilt with each hard bump
* Check Flipper Strength, ensure ball can easily go to top of playfield. Consider Glo Balls.
* Verify balligator works as intended
* Clean Playfield if necessary
* Clean Glass

## Hardware Setup

* 5-Ball Play.

