# Rocket III

## Physical Setup

* Level Machine, per factory recommendation
* Outlane Posts on Medium settings.
* Ear Plug Tilt Hack
* Verify Tilt Sensitivity – should be sensitive, but only one danger with each hard bump
* Verify no flipper disable when coin door opened.
* Check Flipper Strength, ensure ball can easily go to top of playfield.
* Clean Playfield if necessary
* Clean Glass

## Hardware Setup

* 5-Ball Play.
* 
* 6 credits per coin (unless there’s a way to setup free play)
* 