

# Flip Flop

## Physical Setup


* Level Machine, per factory recommendation
* Outlane Posts on Medium settings.
* Ear Plug Tilt Hack if doable
* Verify Tilt Sensitivity – should be sensitive, but only one danger with each hard bump
* Verify no flipper disable when coin door opened.
* Check Flipper Strength, ensure ball can easily go to top of playfield.
* Clean Playfield if necessary
* Clean Glass
* Verify Volume

## Switch or Software Setup


* 5-Ball Play



* Disable Extra Balls, Special worth points (SW6 ON, SW7 ON)



* Max coins per chute



* Low replay score

