# Grand Lizard

## Physical Setup

* Level Machine, slightly steeper than factory recommendation
* Outlane Posts on “Hard Settings”. I.e. most open.
* If possible, place a larger rubber on post adjacent to multiball lock shot.
* Ear Plug Tilt Hack
* Verify Tilt Sensitivity – should be sensitive, but only one danger with each hard bump
* Verify coin door ball save or no flipper disable when coin door opened.
* Check Flipper Strength, ensure ball can easily go up ramps from stopped ball.
* Clean Playfield if necessary
* Clean Glass
* Verify Volume

## Standard Adjustments

* #55 Install 3 Ball
* #64 Install Hard
* #9 Balls per game: 3
* #11 Max EB: 0
* #23 Free Play

## Posted Notes

* TBD