# F14 Tomcat

## Physical Setup

* Level Machine: factory recommended steepness
* Outlane Posts on “Medium Settings”. I.e. MIDDLE position
* Ear Plug Tilt Hack
* Verify Tilt Sensitivity – should be sensitive, but only one danger with each hard bump
* Verify no flipper disable when coin door opened. Fix if needed.
* Check Flipper Strength
* Clean Playfield if necessary
* Clean Glass
* Verify Volume

Game Adjustments:

* #64 INSTALL HARD
* #61 INSTALL NOVELTY
* #7 Special award: POINTS.
* #23 Free Play: ON

Posted Notes: