# Corvette

## Physical Setup

* Level Machine
* Outlane Posts on “Hard Settings”. I.e. most open.
* Check if flippers go dead on coin door open. If yes, disable coin door switch.
* Verify Tilt Sensitivity
* Check Flipper Strength

## Software Setup

Start with UTILS Menu, U.8 Factory Reset

* U.9 Install Medium.
* U.9-10 Install Novelty
* Reset HSTD

Standard Adjustments:

* #A1-02 Tilt Warnings: 1
* #A1-04 Max EBs: 0
* #A1-15 Special: POINTS
* #A1-26 Tournament Play: YES
* #A2-01 Buy-in: OFF
* #A2-05 Ball Save: NONE
* #A2-07 Lock Difficulty: HARD
* #A2-11 Super Skill Shot: OFF
* #A2-12 Challenge Flips: NO
* #A1-33 Game Restart: NEVER
* #A3-17 Free Play: YES

Feature Adjustments:

* Review features if any need to be modified
* HSTD default scores, make them low