# Road Show

## Physical Setup

* Level Machine
* Outlane Posts on “Hard Settings”. I.e. most open.
* Verify Tilt Sensitivity
* Check coin door killing flippers.
* Check Flipper Strength

## Software Setup

* U8 Reset to Factory Default.
* U9-10 Install Novelty
* A3-17 Free Play: ON
* U3 Reset HSTD

Standard Adjustments:

* A1-03 Extra Ball Limit: NO EXTRA BALLS.
* A1-02: 2 tilt warnings
* A1-26, A2-01 Tournament/Competition Mode
* A1-33 Game Restart: NO
* A2-17: No Ball Save
* No buy-in
* Disable coin door switch if necessary.

Feature Adjustments:

* A4-10-14 HSTD default scores, make them low
* Review Other Feature Adjustments