# Scared Stiff

## Physical Setup

* Level Machine slightly steeper than factory recommendation
* Outlane Posts on “Hard Settings”. I.e. most open.
* Remove rubber on movable outlane posts, but keep on post between inlane/outlane
* Ear Plug Tilt Hack
* Verify Tilt Sensitivity – should be sensitive, but only one danger with each hard bump
* Verify no flipper disable when coin door opened. Fix if needed.
* Check Flipper Strength
* Clean Playfield if necessary
* Clean Glass
* Verify Volume

## Software Setup – Utilities, in order:

* U9.07 Install 3-ball
* U9.04 Install Hard.
* U9.10 Install Novelty. (No EB, Special is points)

## Adjustments, after Utilities

* Verify A1-03 No Extra Balls
* A1.26 Tournament Play YES
* A1.33 Game Restart: Never
* A2.01: No buy-in
* A2.08: Ball Saves: 3
* A2.09: Ball Save Time: 3 seconds
* A2.10: Coffin Ball Save: OFF
* A2.11: Crate Ball Save: OFF
* [Dave, verify compensation if Coffin disabled]

## Posted Notes

* No Multiball Ball Saves