# Rocky & Bullwinkle

## Physical Setup

* Level Machine
* Outlane Posts on “Hard Settings”. I.e. most open.
* Verify Tilt Sensitivity
* Check coin door killing flippers.
* Check Flipper Strength

## Software Setup

* A53 Reset to Factory Default.
* A45 Tournament/Competition Mode – Pinball Expo

Standard Adjustments:

* Special award: POINTS.
* A4, A6 Extra Ball Limit: NO EXTRA BALLS.
* A32 Free Play: ON
* A16 2 tilt warnings
* A40 No buy-in
* A41 Game Restart: NO
* Ball Save Time: 3
* Disable coin door switch if necessary.
* Player Competition: YES
* A48 Easy Spot BOMB
* A49 Easy triball restart
* A50 Jackpot Easy
* A51 Yes
* A52 Easy Save Nell
* A24-29 HSTD default scores, make them low
* A12 Reset HSTD, A19 YES

Feature Adjustments:

* TBD