# Gottlieb Counterforce

## Physical Setup

* Level Machine – about 1% steeper than factory recommendation
* Ear Plug Tilt Hack
* Verify Tilt Sensitivity – should be sensitive, but only one danger with each hard bump
* Check Flipper Strength, Consider Glo Balls if playing too slow or can’t hit upper playfield
* Clean/wax playfield
* Clean glass

## Switch or Software Setup

* 3-Ball Play.
* Disable Extra Balls
* Special worth points
* Free Play if possible, else Max Credits per coin
* VERIFY SWITCHES IN MANUAL – This is from same-era Gottlieb, not Counterforce. Mark corrections here.
* 