# Frankenstein

## Physical Setup

* Level Machine, slightly steeper than factory recommendation
* Outlane Posts on “Hard Settings”. I.e. most open.
* Ear Plug Tilt Hack
* Verify Tilt Sensitivity – should be sensitive, but only one danger with each hard bump
* Verify coin door ball save or no flipper disable when coin door opened.
* After #34 adjustment, Check Flipper Strength, ensure right ramp is easily hittable from stopped ball.
* Clean Playfield if necessary
* Clean Glass
* Verify Volume

## Software Setup

* #7 Install HARD.

Standard Adjustments after Software Setup

* #5 Limit Freegame 0
* #6 Limit Extra Balls 0
* #14 Balls Per Game 3
* #30 Free Play ON
* #34 Coil Pulse Power to HARD
* #35 Guaranteed Game Time: 0:00
* #37 Buy-in OFF
* #39 Game Restart: NO
* #43 Player Competition: PAPA
* #47 Laser Kick EXHARD
* #50 Multiball Restart: HARD
* #53 Multiball Difficulty: HARD
* #56 Easy 2-Ball Start: NO

## Posted Notes

* Kickback is UNLIT at start of each ball.