# Sega Godzilla

## Physical Setup

* Level Machine, 1% steeper than factory recommendation
* Outlane Posts on “Hard Settings”. I.e. most open.
* Ear Plug Tilt Hack
* Verify Tilt Sensitivity – should be sensitive, but only one danger with each hard bump
* Verify no flipper disable when coin door opened. Fix if needed.
* After #37 adjustment, Check Flipper Strength, verify ramps are hittable with ease from stopped ball
* Clean Playfield if necessary
* Clean Glass
* Verify Volume

## Software Setup

* #6 Install HARD.
* #44 PAPA Tournament Style. (Sets free play and novelty)

## Standard Adjustments after Software Setup

* #5 OFF – No Extra Balls
* #12 3 Balls per game
* #37 Coil Pulse Power to HARD
* #41 NO Restart Game
* #50 Always Divert to Pops YES