# Stern Terminator 3

## Physical Setup

* Level Machine: 1% steeper than factory recommended
* Outlane Posts on “Hard Settings”. I.e. fully open position
* Remove rubber from movable outlane post, keep it on post between inlane/outlane
* Ear Plug Tilt Hack
* Verify Tilt Sensitivity – should be sensitive, but only one danger with each hard bump
* Verify no flipper disable when coin door opened. Fix if needed.
* Check Flipper Strength, especially for hitting ramps
* Clean Playfield if necessary
* Clean Glass
* Verify Volume

## Install Menu (in order)

* Install Hard
* Install Free Play Competition.
* Install Novelty

## Standard Adjustments, verify or update AFTER “Install Menu”

* #06 Special Limit: POINTS.
* #09 Extra Ball Limit: NO EXTRA BALLS.
* #14 Balls per Game: 3
* #30 Free Play: YES
* #33 Coil Power: HARD (verify machine plays ok)
* #35 Game Restart: NO
* #38 Freeze Save Time: 3
* #40 Timed Plunger OFF
* #41 Flipper Ball Launch DISABLED
* #42 Coin Door Ball Saver: YES
* #43 Competition Mode: YES
* #44 Consolation Ball: NO
* #48 Player Competition: NO

Feature Adjustments:

* #03 Start Multiball Diff: EXHARD
* #05 Kickback Relight Diff: EXHARD
* #09 Disable RPG: YES.
* #11 Adult Content: NO.
* Disable/Reduce Multiball Ball Saver if possible.

Posted Notes:

RPG Disabled – 5M Points. [verify]